Flat Handover & Snag Inspection Checklist
Tamil Nadu · Jumbo Realty
Use this when the builder invites you to take possession. Inspect before you sign the possession letter, list every defect in writing, and keep dated photos. Take a friend or an engineer if you can.
Documents to collect
☐  Possession letter, with the handover date
☐  Copy of your registered sale deed (and construction agreement, if separate)
☐  Completion / occupancy certificate for the building, as applicable to the project
☐  Receipts for every payment made, including GST, car parking, corpus and maintenance deposits
☐  Electricity (EB) and water / sewer connection details, and the process to move them to your name
☐  Property tax assessment details, and how to transfer it to your name
☐  Warranty cards and invoices for lifts, fittings, appliances or equipment supplied with the flat
☐  Final approved floor plan and the carpet area stated in your agreement
☐  Owners' association contact details and maintenance terms
Walls, ceilings & floors
☐  No cracks, dampness or seepage marks, especially near bathrooms, kitchen and external walls
☐  Even paint finish; no patches or peeling
☐  Floor tiles level, not hollow when tapped, no chips or cracks; even grout lines
☐  Skirting fixed properly all around
Doors & windows
☐  Doors open, close and lock smoothly; locks and keys work
☐  Windows slide or open freely; no gaps; glass not cracked
☐  Grills and safety grills fixed and painted
☐  Balcony door and railings firm; railing height feels safe
Plumbing
☐  Every tap and shower: good pressure, hot and cold where provided
☐  No leaks under sinks, around WCs or at joints
☐  Floor slopes towards the drain in bathrooms and balconies; water does not pool
☐  WCs flush properly; geyser points and water heater connections in place
Electrical
☐  Every switch, socket, light and fan point works (carry a small tester or phone charger)
☐  Distribution board labelled; MCBs / ELCB in place
☐  AC points, geyser points and kitchen appliance points as per plan
☐  Earthing in place; no exposed wiring
Kitchen & utility
☐  Counter firm, no cracks; sink and drain work
☐  Space and points for chimney, water purifier and appliances as promised
☐  Utility area tap and drain work
Common areas
☐  Lift works; backup power for lift and common areas
☐  Allotted car parking marked as per agreement
☐  Amenities promised in the brochure / agreement are complete and working
☐  Fire safety equipment installed in corridors and staircases
Snag list (defects to be fixed)
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Note: Give the snag list to the builder in writing and keep their acknowledgement. Under section 14(3) of the RERA Act, 2016, if a structural defect, or a defect in workmanship, quality or services, is brought to the builder's notice within five years of possession, the builder must fix it without charge within 30 days.
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